Thermal Controller LED operation V1.7

|  |  |  |
| --- | --- | --- |
| **LED** | **Color** | **Operation** |
| LED 1 – Serial COM | White | Toggles on/off every time a successful command was sent/received from Athena. Solid White on communication failure to Athena |
| Led 2- Fan Status | Green | Green indicates Fan is on |
| Led 3 | White | Not implemented |
| Led 4 –USB status | Green | Blinks green on successful USB connection. Solid green on USB failure |